(footprint "Jack_STX-3000"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 8.5 -4.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7b0b7c8f-69f2-42ca-9bbf-cc1b925c575d")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "STX-3000"
		(at 7.5 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "875a2ea9-dc5e-45a3-9c7c-791ef460e621")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.kycon.com/Pub_Eng_Draw/STX-3000.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "064682f4-799f-4eb1-8170-44a8ec114203")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9984d51a-5961-4902-b3eb-c018cbf6c537")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start 0 -3)
		(end 1.9 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "faeb69b9-c1be-4043-8bb7-497dbcbdbb25")
	)
	(fp_rect
		(start 1.9 -3.6)
		(end 14 3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "38d5393e-5f96-48bb-b3f0-f7641b1f3034")
	)
	(fp_rect
		(start -0.5 -4)
		(end 14.5 4)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "9ef12da9-2306-4964-976d-3165fca70ec0")
	)
	(fp_rect
		(start 0 -3)
		(end 1.9 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "3ef1b056-ee1a-48b1-b005-8383810a7511")
	)
	(fp_rect
		(start 1.9 -3.6)
		(end 14 3.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "04dc7a4b-6170-4d0e-82b9-2b1ee44d80a3")
	)
	(fp_text user "${REFERENCE}"
		(at 7.5 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "05a7b942-0bbe-4196-9dc9-2f5d24bf759b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 4 0)
		(size 0.1 0.1)
		(drill 1)
		(layers "*.Mask")
		(uuid "6073c2e6-e4c0-4b5c-a1ca-afa87fe96fa7")
	)
	(pad "" np_thru_hole circle
		(at 11.5 0)
		(size 0.1 0.1)
		(drill 1)
		(layers "*.Mask")
		(uuid "68ab71eb-f318-46b9-a7fe-63ba8047c582")
	)
	(pad "R" thru_hole rect
		(at 13.4 -2.75)
		(size 1.9 1.4)
		(drill oval 1.5 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fd21e004-dac6-4c3d-8596-54ed017d3cd3")
	)
	(pad "S" thru_hole rect
		(at 13.4 2.75)
		(size 1.9 1.4)
		(drill oval 1.5 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7c663d28-6208-45e9-8211-94daa3709903")
	)
	(pad "T" thru_hole rect
		(at 8.1 1.5)
		(size 1.9 1.4)
		(drill oval 1.5 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "31320170-2cb0-4d6e-bec2-502870004db0")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/STX-3000_rD3.IGS"
		(offset
			(xyz 1.9 3.6 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 90)
		)
	)
)
