(footprint "Ultrasound_Transmitter_USO16A12TLFPM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -10.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "33675a0a-e3a8-4957-9fa1-7de197f39116")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "USO16A12TLFPM"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7f8d304e-8c02-499a-a535-d55167a649bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "44ebc587-edb4-4365-9b44-b4fb64b45d0a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e7cb780-0992-4dd1-82a7-a75dc88a86ad")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 8.1 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "bf30c783-5c8f-4ba8-b13b-084f635b2195")
	)
	(fp_circle
		(center 0 0)
		(end 0 -9)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "0d47d60e-3a8b-434b-827a-85aad80dbad2")
	)
	(fp_circle
		(center 0 0)
		(end 0 -8.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "2163e83e-aaa3-4161-aef7-eb5aa6be8aa1")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "48a61ae4-e58a-4e81-9ad3-151fda0ba21e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -5 0)
		(size 1.8 1.8)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "701f98de-5684-4fc3-9f02-276282dd4852")
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 1.8 1.8)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3250a44e-c97d-4ad2-9c3b-58c772252ced")
	)
	(embedded_fonts no)
)
