(footprint "Battery_BC3AAPC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5c0949d8-9c84-4400-a195-d7acbbc60606")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "BC3AAPC"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e4ab3482-c1c7-4990-8fad-10f86f1db5be")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "25d5815e-d35b-4e66-b5c9-f67308e77114")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c49bf088-236a-4a1c-a47d-7832d02eb574")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -28.9 -39)
		(end 28.9 8.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "6aea6589-02c7-495e-934b-fa4d0baba552")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "84dba0ac-527b-42c9-abc7-ba3ab71eea24")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 -30)
		(size 2.37 2.37)
		(drill 2.37)
		(layers "F&B.Cu" "*.Mask")
		(uuid "567ac1de-10fe-4d76-a826-6781680fea56")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 2.37 2.37)
		(drill 2.37)
		(layers "F&B.Cu" "*.Mask")
		(uuid "65aaf9ce-2e34-4ab3-a95c-5d5cbb87607d")
	)
	(pad "1" thru_hole circle
		(at 26.07 -12.8)
		(size 1.5 1.5)
		(drill 1.17)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a5d8c983-6f0d-4b06-b331-70d6051990e2")
	)
	(pad "2" thru_hole circle
		(at 26.07 0)
		(size 1.5 1.5)
		(drill 1.17)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f0ec3fe-094f-4955-8393-2ca4eadd36f3")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/BC3AAPC_BC3AAPC.STEP"
		(offset
			(xyz -0.25 -1.4 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -180)
		)
	)
)
